|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Element/ Str. Unit No.** | **Element/Structure Unit Description** | **Total Qty** | **Units** | **Condition State Quantity** | | | |
| **CS 1** | **CS 2** | **CS 3** | **CS 4** |
| **1** | **Span(s) - All** |  |  |  |  |  |  |
| **DECK/SLAB** | |  |  |  |  |  |  |
| 12 | RC Deck | 4500 | sq. ft. |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **JOINTS** |  |  |  |  |  |  |  |
| 300 | Strip Seal Expansion Joint | 60 | ft. |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **APPROACH SLABS** | |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **BRIDGE RAILINGS** | |  |  |  |  |  |  |
| 330 | Metal Bridge Railing | 300 | ft. |  |  |  |  |
| 331 | RC Bridge Railing | 300 | ft. |  |  |  |  |
| **SUPERSTRUCTURE** | |  |  |  |  |  |  |
| 107 | Steel Open Girder/Beam | 864 | ft. |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 515 | Steel Protective Coating | 8640 | sq. ft. |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **BEARINGS** | |  |  |  |  |  |  |
| 311 | Movable Bearing | 12 | each |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 515 | Steel Protective Coating | 48 | sq. ft. |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 313 | Fixed Bearing | 12 | each |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 515 | Steel Protective Coating | 48 | sq. ft. |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **SUBSTRUCTURE** | |  |  |  |  |  |  |
| 210 | RC Pier Wall | 30 | ft. |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 215 | RC Abutment | 60 | ft. |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |